 Electronic Notes in Theoretical Computer Science 203 (2008) 111–124 

[www.elsevier.com/locate/entcs](http://www.elsevier.com/locate/entcs)

Extending Lustre with Timeout Automata

Jimin Gao[a](#_bookmark0)*,*[1](#_bookmark2) *,*[2](#_bookmark2) Mike Whalen[b](#_bookmark1)*,*[3](#_bookmark2) Eric Van Wyk[a](#_bookmark0)*,*[1](#_bookmark2) *,*[4](#_bookmark2)

a *Department of Computer Science and Engineering University of Minnesota*

*Minneapolis, MN, USA*

b *Advanced Technology Center Rockwell Collins, Inc.*

*Cedar Rapids, IA, USA*

Abstract

This paper describes an extension to Lustre to support the analysis of globally asynchronous, locally syn- chronous (GALS) architectures. This extension consists of constructs for directly specifying the *timeout automata* used to describe asynchronous communication between processes represented by Lustre nodes. It is implemented using an extensible language framework based on attribute grammars that allows such extensions to be modularly defined so that they may be more easily composed with other language exten- sions.

*Keywords:* synchronous languages, extensible languages, attribute grammars, composable language extensions

# Introduction

Synchronous languages [[2](#_bookmark16)] have been successfully used to describe and reason about a wide variety of systems, including hardware design and synthesis [[24](#_bookmark39)], embedded software control [[2](#_bookmark16)], and modeling and analysis of globally asynchronous, locally synchronous (GALS) architectures [[15](#_bookmark30)]. These can be seen as *domain-speciﬁc lan- guages* that address the concurrency and synchronization concerns of embedded systems and hardware at a high-level of abstraction.

The Lustre language [[14](#_bookmark29)], in particular, has been used in a wide range of aca- demic and industrial projects. To better suit specific communities, the Lustre lan- guage has evolved into different dialects that further specialize the language. These

1 This work is partially funded by NSF CAREER Award #0347860, NSF CCF Award #0429640, and the McKnight Foundation.

2 Email: [jgao@cs.umn.edu](mailto:jgao@cs.umn.edu)

3 Email: [mwwhalen@rockwellcollins.com](mailto:mwwhalen@rockwellcollins.com)

4 Email: [evw@cs.umn.edu](mailto:evw@cs.umn.edu)

1571-0661 © 2008 Elsevier B.V. Open access under [CC BY-NC-ND license](http://creativecommons.org/licenses/by-nc-nd/3.0/).

doi:10.1016/j.entcs.2008.05.014

dialects have evolved from a simple “kernel” language that has been fairly stable throughout the development of Lustre. For example, to better support safety- critical software development, activation conditions (condact) and initialized delay (fby) constructs were added to the variant of the language used by the SCADE toolset [[11](#_bookmark26)], and a richer type system and modularity constructs have been pro- posed in Lustre v6. Other examples include with expressions and array slicing and composition operators in Lustre v4, case, TO and FROM expressions and support for generic types in the SCADE textual syntax, and different packages for statecharts-like extensions to the language [[8](#_bookmark21),[20](#_bookmark35)]. In recent work [[12](#_bookmark27)], we have ex-

−*e*

tended Lustre with condition tables like those found in RSML [[25](#_bookmark40)], state variables

for building simple state machines, and a notion of events.

There are many more domain-specific features that would make Lustre easier to use in new domains. For example, Lustre has been used for the analysis [[15](#_bookmark30)] and code generation [[5](#_bookmark20),[6](#_bookmark22)] of GALS architectures. Our interests here are in using Lustre to specify and analyze (but not generate code from) the behavior of GALS architec- tures. Previous explorations of this idea, such as [[15](#_bookmark30)], assume that users manually construct a scheduler node and use it to manage the clocks of all of the asynchronous processes in the model. However, a scheduler could be automatically derived using a language extension, given the rates and drift of the asynchronous processes in the model. To support this process, we add to Lustre a *timeout condact* construct that defines the behavior of an asynchronous process within the architecture as follows:

*a, b* = *timeout condact* (*rate, min drift, max drift, channel* (*x , y* )*, init a, init b*);

This construct (defined in Section [2](#_bookmark4)) specifies that node *channel* representing a periodic process within the architecture is to be executed every *rate* milliseconds subject to clock drift in the range *min drift ..max drift* . Like a *condact* expression, if the node does not evaluate, then the result of the expression is the value from the most recent evaluation, and before the first evaluation, the values *init a* and *init b* are used. Using this construct, a scheduler (implemented in the kernel Lustre language) can be automatically derived.

Extending a language using traditional techniques often requires a large de- velopment and tooling effort. Thus, there has been much research in programming languages communities on the development of techniques and tools for implementing languages that reduce the costs associated with adding new features to languages. There are (at least) two important criteria for extensions to a language. First, the new language constructs should have the same “look and feel” as the host language constructs. That is, they should support the same type of error-checking, optimiza- tion, and translations as do the host language constructs. Second, it should be pos- sible to combine implementations of different extensions to the same host language to create a new language which incorporates the constructs in both. Furthermore, such a composition should require little or no implementation-level knowledge of the language extensions. When this second criteria (referred to as the “composability criteria”) is not met, users may be forced to chose between incompatible dialects of Lustre that individually have only some of the desired language constructs.

In previous work [[28](#_bookmark43)], we raised this issue of incompatible dialects and the tra-

ditionally high cost of language development. We proposed an extensible language framework for Lustre based on attribute grammars as a possible alternative ap- proach to language development that satisfies the two criteria mentioned above. This approach is used to implement timeout automata as language constructs in Lustre. The primary contributions of this paper are the specification and implemen- tation of timeout automata as first class language constructs in Lustre. Section [2](#_bookmark4) describes the GALS approach to development and defines the timeout automata construct. Section [3](#_bookmark11) describes some aspects of the implementation of the timeout automata as a language extension in our extensible languages approach. Section [4](#_bookmark15) discusses related work and concludes.

# Timeout Automata and GALS architectures

* 1. *GALS and Flight Guidance Synchronization Example*

To illustrate our approach to the analysis of GALS architectures, we describe the synchronization logic in a Flight Guidance System (FGS). The FGS compares the measured state of the aircraft (position, speed, and attitude) to the desired state and generates pitch and roll guidance commands to minimize the difference be- tween the measured and desired state. The FGS subsystem accepts input about the aircraft’s state from several other subsystems and computes the pitch and roll guidance commands provided to the autopilot.

The FGS system has two physical sides corresponding to the left and right sides of the aircraft. These provide redundant implementations that communicate over a cross-channel bus. Normally, only one FGS instance (the pilot flying side) is active, with the other FGS instance operating as a silent, hot spare. A *transfer switch* button on the flight control panel (FCP) can be used to toggle the pilot flying side. In some critical flight modes, both sides are active and independently generate guidance values for the autopilot, so that the autopilot can verify that they agree within a predefined tolerance value. [5](#_bookmark5)






To make the example of this paper tractable, we restrict ourselves to a simplified specification that deals only with the logic determining whether an FGS instance is active. This example captures critical functionality for the FGS, e.g., at least one side is active at all times, and illustrates some of the communication and coordi- nation problems that can occur in GALS systems. In our analysis [[21](#_bookmark36)], we prove that this simplified model simulates the behavior of the full FGS w.r.t. synchro- nization, thereby ensuring that the results proven about the simplified specification also apply to the full specification.

A graphical model of the system architecture is shown in Figure [1](#_bookmark6). The system inputs are:

* + - the *Transfer Switch* input (1), which switches the *pilot flying* side,
    - the *Independent Mode* inputs (2, 3), which are Boolean signals that determine

5 A more detailed description of the FGS can be found in [[21](#_bookmark36)].

Fig. 1. Two FGS Synchronization Architecture in Simulink



whether each side believes it is in the independent mode of operation, [6](#_bookmark8) and

* the *Clock* inputs (4 – 7). Clocks are Boolean signals that enable the execution of the processes within the architecture. Treating the clock signals as unconstrained inputs allows us to model GALS systems within a synchronous paradigm [[15](#_bookmark30)]. By embedding this model inside a model that constrains the clocks, we can model a variety of different physical architectures and reason about their behavior.

The system outputs are:

* the *Active* outputs, which are Boolean signals that describe whether each side be- lieves itself to be active, i.e., computing pitch and roll commands for the autopilot, and
* the *Pilot Flying* outputs, which are Boolean signals that describe whether each side believes itself to be the pilot flying side.
  1. *Timeout Automata*

A *timeout automaton* is a mechanism for constraining the Boolean clocks of processes to match a notion of real (calendar) time. As described in [[9](#_bookmark23)], the automata consists of a set of processes, each of which run at a certain rate. A *scheduler* (also called an event list) stores the times at which each of the processes will next execute. Evaluation of the system consists of advancing time to the next instant in which a process (or processes) can execute. Given a set of processes *P* , we assume that each process *p* ∈ *P* has an associated rate *rp*, a time until next execution *tp*, and a Boolean clock signal *cp*, and that there is a distinguished variable *ci* that records the increment of time since the last instant. Then, given a state *σ* mapping identifiers to values, we generate a new state *σ*' as follows:

6 As discussed in [[21](#_bookmark36)], in an actual system these are not inputs to the FGS but are instead computed. However, the system synchronization properties do not depend on the details of this computation.

* + - *σ*'(*ci*) equals min(*σ*(*t* )) where *p* ∈ *P*

*p*

* + - *σ*'(*c* ) is true iff *σ*'(*ci*) − *σ*(*t* )= 0

*p p*

* + - *σ*'(*t* ) equals *r* if *σ*'(*c* ); otherwise *σ*'(*ci*) − *σ*(*t* ).

*p p p p*

Each process “fires” (executes) when its clock signal *cp* is true. Time always advances by some positive increment described by *ci*. If multiple processes share the same value for *tp* and *tp* = *ci*, then they execute simultaneously within the step. Clock drift between processes can be introduced to the model by allowing the rate *rp* of each process to vary within some specified range.

In [[9](#_bookmark23),[3](#_bookmark18),[4](#_bookmark19)] this approach has been shown to be amenable to model-checking using SMT-based solvers for interesting GALS problems. We have also used it for system simulation and testing. The primary advantage of timeout automata for analysis that maximal time progress is made on each step (i.e., there are no “stuttering” steps in which the clock ticks but no other changes occur), and each step consumes a varying amount of real time as described by the clock increment *ci*.

In the Dual FGS example, we have used timeout automata to prove the correct- ness of the synchronization logic between the two FGSs. Properties proved include:

(1) at least one FGS is always *Active*, and (2) at most one FGS is the *Pilot Flying* side. Other properties of interest are described in [[21](#_bookmark36)]. The proofs follow the process described in [[9](#_bookmark23)].

* 1. *Implementation of Timeout Automata In Lustre*

Timeout automata can be described as an extension to Lustre with the addition of a new expression construct:

*timeout condact* (*rate, min drift, max drift,* ⟨*node*⟩*,* ⟨*init vals*⟩);

This construct specifies that node *node* representing a periodic process within the architecture is to be executed every *rate* milliseconds subject to clock drift in the range *min drift ..max drift* . Like a *condact* expression, if the node does not evaluate, then the result of the expression is the value from the most recent evaluation, and before the first evaluation of the node, the initial values *init vals* are used. It is assumed (and checked by the compiler) that *timeout condact* expressions are not nested within other clocked expressions; this matches the expectation within GALS systems in that the asynchrony occurs at the global level and synchronous clocking mechanisms are local to one of the modeled processes.

In the Dual FGS model, the left and right FGSs run every 100 ms with a +/- 1 ms drift and communications between the two FGSs requires 15 to 25 ms. The expression of this architecture in Lustre is shown in Figure [2](#_bookmark9).

The semantics of the timeout condact specifications match the formalization in Section [2.2](#_bookmark7). Each timeout condact expression becomes a process in the timeout automata model, and a global scheduler is synthesized in Lustre from the set of these processes. As an example, consider Figure [3](#_bookmark10), the automatically generated implementation in Lustre for the FGS timeout condact in Figure [2](#_bookmark9).

type fgs\_data = ... ; /\* contains PF, Independent, and Ack data \*/ const lft\_fgs\_init = ... ; lr\_init = ... ;

rht\_fgs\_init = ... ; rl\_init = ... ;

node fgs ( other\_fgs\_in: fgs\_data, ind\_mode: bool, transfer\_switch: bool, init\_pilot\_flying: bool)

returns ( fgs\_out: fgs\_data ) ; let ... tel ;

node channel ( channel\_in: fgs\_data) returns ( channel\_out: fgs\_data ) ;

let ... tel ;

node main ( trans: bool, lft\_ind\_mode: bool, rht\_ind\_mode: bool ) returns ( lft\_fgs\_pilot: bool, lft\_fgs\_active: bool,

rht\_fgs\_pilot: bool, rht\_fgs\_active: bool ) ;

var

lft\_fgs\_out: fgs\_data ; lr\_chan\_out: fgs\_data ; rht\_fgs\_out: fgs\_data ; rl\_chan\_out: fgs\_data ;

let

1. lft\_fgs\_out = timeout\_condact(100.0, -1.0, 1.0,

fgs(rl\_chan\_out, trans, lft\_ind\_mode , true), lft\_fgs\_init) ;

1. lr\_chan\_out = timeout\_condact(20.0, -5.0, 5.0,

channel(lft\_fgs\_out),lr\_init);

1. rht\_fgs\_out = timeout\_condact(100.0, -1.0, 1.0,

fgs(lr\_chan\_out, trans, rht\_ind\_mode , false), rht\_fgs\_init) ;

1. rl\_chan\_out = timeout\_condact(20.0, -5.0, 5.0,

channel(rht\_fgs\_out),rl\_init);

tel;

Fig. 2. FGS Synchronization Architecture using timeout condact.

The timeout node (line 8 of Figure [3](#_bookmark10)) is used to define the *rp*, *cp*, and *tp* variables for a process within the model. The rate and drift inputs set *rp*, the init time input sets the initial value of *tp*, and the time decrement input corresponds to the global time decrement between steps *ci*. The timeout node contains an individual count-down timer time remaining that corresponds to *tp*, and generates a Boolean signal fired that corresponds to *cp*.

The expansion of the timeout condacts in main creates instances of the timeout node for each process and define constraints that describe the legal values for timers and drift inputs within the model. Line (3) in Figure [3](#_bookmark10) is the translation of the first timeout condact in Figure [2](#_bookmark9) to its implementation as a kernel language condact construct. The component node call to fgs and the initial values are the same; but the rate and drift parameters have been replaced by a clock variable (corresponding to *cp* in the formal model) named fired 1. This variable is set on line (6) by a call to the timeout node that implements the time keeping operations of the timeout condacts.

On Figure [3](#_bookmark10) line (7), the model then selects the smallest time-remaining as the amount to advance each component clock (time decrement) and feeds that value back to each individual component timer for use in computing the next clock tick. The definition of the node min is not shown but is what one would expect. Since the time decrement value specifies the elapsed global time since the last clock tick, it is also output from the main node to allow a model checker to check properties involving global time (for example, the maximum time that some property *P* can be false is less than some time *t*).

Assert statements are also generated to restrict the new input drift values to be within the originally specified ranges of possible clock drift specified in the original

node main (drift\_4: real, init\_time\_4: real, drift\_3: real, init\_time\_3: real, drift\_2: real, init\_time\_2: real, drift\_1: real, init\_time\_1: real, trans: bool, lft\_ind\_mode: bool, rht\_ind\_mode: bool)

returns (time\_decrement: real,

lft\_fgs\_pilot: bool, lft\_fgs\_active: bool, rht\_fgs\_pilot: bool, rht\_fgs\_active: bool);

* 1. var fired\_4: real; time\_remaining\_4: real; fired\_3: real; time\_remaining\_3: real; fired\_2: real; time\_remaining\_2: real; fired\_1: real; time\_remaining\_1: real;
  2. lft\_fgs\_out: fgs\_data ; lr\_chan\_out: fgs\_data ; rht\_fgs\_out: fgs\_data ; rl\_chan\_out: fgs\_data ;

let

* 1. lft\_fgs\_out = condact(fired\_1, fgs(rl\_chan\_out, trans,lft\_ind\_mode, true),

lft\_fgs\_init);

lr\_chan\_out = condact(fired\_2, channel(lft\_fgs\_out), lr\_init);

rht\_fgs\_out = condact(fired\_3, fgs(lr\_chan\_out, trans,rht\_ind\_mode, false),

rht\_fgs\_init);

rl\_chan\_out = condact(fired\_4, channel(rht\_fgs\_out), rl\_init);

* 1. assert(((drift\_1 <= 1) && (drift\_1 >= -1)));
  2. assert(((init\_time\_1 >= 0.0) && (init\_time\_1 <= (100.0 + 1)))); assert(((drift\_2 <= 5) && (drift\_2 >= -5))); assert(((init\_time\_2 >= 0.0) && (init\_time\_2 <= (20.0 + 5)))); assert(((drift\_3 <= 1) && (drift\_3 >= -1))); assert(((init\_time\_3 >= 0.0) && (init\_time\_3 <= (100.0 + 1)))); assert(((drift\_4 <= 5) && (drift\_4 >= -5))); assert(((init\_time\_4 >= 0.0) && (init\_time\_4 <= (20.0 + 5))));
  3. fired\_1, time\_remaining\_1 = timeout(100.0, drift\_1, init\_time\_1,

time\_decrement);

fired\_2, time\_remaining\_2 = timeout(20.0, drift\_2, init\_time\_2,

time\_decrement);

fired\_3, time\_remaining\_3 = timeout(100.0, drift\_3, init\_time\_3,

time\_decrement);

fired\_4, time\_remaining\_4 = timeout(20.0, drift\_4, init\_time\_4,

time\_decrement);

* 1. time\_decrement = min(time\_remaining\_4, min(time\_remaining\_3,

min(time\_remaining\_2, time\_remaining\_1)));

tel;

* 1. node timeout (rate: real, drift: real, init\_time: real, time\_decrement: real)

returns (fired: real, time\_remaining: real); let

time\_remaining = init\_time -> if fired then rate + drift

else pre(time\_remaining) - pre(time\_decrement); fired = (pre(time\_remaining) <= pre(time\_decrement));

tel;

Fig. 3. Translated FGS Timeout Automata Model

timeout condact constructs. For the first timeout condact, the generated assert statements are shown in Figure [3](#_bookmark10) lines (4) and (5). Additional input parameters for the unconstrained input drift values are also added to the interface of main. The translation also adds new local variables in the line following the label (1).

The translation of the timeout condact constructs involves more that just local transformations that are possible with macro processing. The translation needs to generate new equations for each timeout condact and for defining time decrement based on a global analysis that determines how many timeout condacts were used in the original code and what the generated time-remaining variables for each one are. Note that the original type declarations for fgs data, the four constant *init* values and the declarations of the fgs and channel nodes are not changed in the translation and appear in the translated code as they did in the original. Thus, they are not repeated in Figure [3](#_bookmark10).

As there are only four processes in this model, the automata is relatively simple. However, with larger number of processes, it can become unwieldy. It is “boiler- plate” code that must be re-written for each GALS system to be analyzed. Also,

it is cumbersome to experiment with different architectural configurations (e.g., changing the rates and drift) in the translated model. We wish to encourage this kind of experimentation and formal analysis in the early stages of system design. Finally, there are hints that can be provided to aid analysis based on the structure of the automata (for example, the minimum and maximum possible values that the system clock can advance within a step). To make it easy to analyze these kinds of models, we would prefer to add a language construct to automatically construct the automata.

# Timeout Automata as a Language Extension

Implementing the timeout automata described in Section [2](#_bookmark4) by translation to the kernel Lustre language does not, per se, pose any exceptionally difficult challenges. Any solution, including ours, will (*i*) add a timeout node like the one in Figure [3](#_bookmark10) to the specification, (*ii*) add the equations that call to the timeout node and cal- culate the time decrement value, and (*iii*) replace all timeout condact constructs with the appropriate condact constructs that use the new Boolean *ﬁred* flag. The main challenges arise in satisfying the look-and-feel and composability criteria de- scribed in Section [1](#_bookmark3). We have built [[12](#_bookmark27)] an extensible language framework based on higher-order attribute grammars (AGs) [[17](#_bookmark32),[30](#_bookmark44)] and implemented an AG speci- fication language called Silver [[26](#_bookmark41)] that supports the building of languages and ex- tensions that satisfy these criteria. In this approach a host language and language extensions are implemented as individual Silver AG modules. The supporting tools allow the composition of these modules to define new extended languages with little or no implementation-level knowledge of the host or languages extensions [[12](#_bookmark27)]. In this section we give a brief overview of how the *timeout condact* extension is con- structed using this approach. Due to space constraints this is necessarily cursory and a number of simplifications and omissions have been made, but the full Silver specifications can be found at [www.melt.cs.umn.edu](http://www.melt.cs.umn.edu/).

* 1. *Mini-Lustre as the Host Language*

The specification for Mini-Lustre (a subset of Lustre) is written in Silver, a por- tion of which is shown in Figure. [4](#_bookmark12). A Silver specification for a language consists of an unordered series of declarations that define its concrete and abstract syntax as well as rules which assign values to attributes associated with non-terminals in the abstract syntax tree (AST). Since concrete syntax is defined as expected for traditional parser and scanner generators we do not show those and only discuss abstract syntax. To define the (abstract) syntax, there are declarations for termi- nals, non-terminals (keyword nt), and productions (prod), following standard AG terminology [[17](#_bookmark32)]. Synthesized attributes (syn) propagate information up the ab- stract syntax tree; inherited attributes (inh) propagate information down the AST. Equations defining attribute values are used to specify the semantic analyses, such

as type checking. [7](#_bookmark13)

grammar lustre ;

nt Root, DclList, Dcl, VarDclList, VarDcl, Locals, EqList, Eq, IdList, Expr; syn attr pp :: String occurs on Root, Dcl, Expr, VarDcl, ... ;

syn attr errors :: String occurs on Root, Dcl, Expr, ... ; syn attr ctrans :: String occurs on Root, Dcl, Expr, ... ; syn attr typerep :: TypeRep occurs on Expr, ExprList ;

prod root r::Root ::= dl::DclList

{ r.pp = dl.pp; r.errors = dl.errors; r.ctrans = ... dl.ctrans ...; } prod dclListCons dl::DclList ::= d::Dcl dltail::DclList { ... }

prod dclListOne dl::DclList ::= d::Dcl { ... }

prod nodeDcl n::Dcl ::= name::Id inputs::VarDclList outputs::VarDclList

locals::VarDclList eqs::EqList

{ n.pp = "node " ++ name.lexeme ++ " (" ++ inputs.pp ++ ") " ++ "returns"

++ " (" ++ outputs.pp ++ ") " ++ "\n" ++ locals.pp ++ "\nlet\n"

++ eqs.pp ++ "\ntel;\n";

n.errors = inputs.errors ++ outputs.errors ++ ... ; n.ctrans = ... ; } prod varDcl vd::VarDcl ::= var::Id type::Type { ... }

prod equation eq::Eq ::= ids::IdList expr::Expr

{ eq.pp = ids.pp ++ " = " ++ expr.pp ++ ";\n" ;

eq.errors = ... ; /\* ensure ids and expr have same type(s) \*/ } prod idExpr e::Expr ::= id::Id

{ ...; e.ctrans=...; e.errors = ... ; /\* ensure id is declared \*/ }

prod condactExpr e::Expr ::= f::Expr call::Expr init\_vals::ExprList { ... }

Fig. 4. A portion of the Silver specification of Mini-Lustre.

The first line in Figure [4](#_bookmark12) provides the name of this grammar. These are used in import statements to compose attribute grammar specifications to create the specification for an extended language. Next, are declarations for nonterminals. Synthesized attributes pp, errors, and ctrans of type String are declared; these attributes, respectively, define a node’s pretty-print or “unparsed” representation, the errors occurring on the node and its children, and its translation to C. The attribute typerep is used to represent the type of an expression or expression/id list. The occurs on clause specifies which nonterminals an attribute decorates. We will elide other nonterminal and attribution declarations as they can be inferred from the specification.

A Mini-Lustre program (represented by Root) is a series of declarations (DclList). The nonterminal Root on the left hand side of production root is named r (“::” reads as “has type”); the right hand side has a single DclList nonterminal named dl. Equations defining the synthesized attributes of r are listed in curly brackets. For example, the first equation defines the pp attribute on r to be the value of pp on dl. A node, defined by nodeDcl, has a name (name), a list of input parameter declarations (inputs:: VarDclList), a list of output parameters (outputs), a list of local variable declarations (locals), and a list of equations (eql:: EqList). The production varDcl binds identifier names to types. These bindings are stored in a symbol table that is passed to the equations in eqs and used for type-checking the expressions and equations following rules specified by the errors attributes. For example, the production equation checks that the identifier id and expression expr have the same type and generates an error message if they do not.

7 This is meant broadly and can include causality and initial-state-definedness checks.

* 1. *Timeout Automata as a Language Extension*

To add the *timeout condact* construct to the extensible Lustre framework we must write a Silver attribute grammar specification that will specify the concrete and abstract syntax of the new construct, perform error checking and other analyses on the *timeout condact*, specify its translation to a *condact* construct, and for each use of a *timeout condact* in a node add additional equations and parameters to that node. Further we must add the definitions for the *timeout* and *min* node to the Lustre specification. Using language features provided by Silver, all these tasks can be specified in a single grammar module, thus making this extension a stand- alone unit that can be optionally composed with other similarly-defined language extensions.

Fig. [5](#_bookmark14) shows the Silver production tmoCondactExpr that specifies the abstract syntax of the *timeout condact* construct. To maintain the native look-and-feel, the pp, errors, and typerep attributes are defined explicitly in this production. Explicitly defining errors ensures that type errors are detected and reported on the *timeout condact*, not its kernel Lustre translation. Though elided, the definition of errors checks that the types of values returned by the node call call match the types of the initial values init vals.

Although tmoCondactExpr explicitly defines some attributes, it does not do so for attributes such as ctrans (or attributes for translating to the input languages of different model checkers). These attributes are *implicitly* defined using *forward- ing* [[27](#_bookmark42)] through translation to a *condact* (condactExpr) in the host language by using the forwards to clause. When a tmoCondactExpr node in the AST is queried for an attribute that is not explicitly defined by an attribute definition, it forwards that query to the forwards-to construct. The value defined there is returned as the value of that attribute for the *timeout condact*. Thus, the value of ctrans on a *timeout condact* is the value of the ctrans attribute on the generated (translated- to) *condact* construct. Therefore, all back-end tools only see the generated *condact* calls while Lustre programmers see the *timeout condact* calls they write.

In addition, the Silver specification assigns a unique integer identifier (attribute num) to each *timeout condact* call. The identifier for each call is used in generated lo- cal variable names such as fired 1 and fired 2 as seen in Figure [3](#_bookmark10). Furthermore, relevant information regarding this *timeout condact* call is gathered and propa- gated up the AST to the enclosing node declaration using the synthesized attribute tmoCallInfoList. This information is used for generating the added equations for variables such as time remaining 1 and time decrement also seen in Figure [3](#_bookmark10). The additional attribute definitions of tmoCallInfoList on existing host language productions can be all specified in the grammar module of the *timeout condact* ex- tension by using the Silver language feature *aspect productions*, and no changes to the host language specification need to be made [[13](#_bookmark28)]. Once the information of all *timeout condact* calls in a node is gathered to the level of node declaration (produc- tion nodeDecl), it is used to generate additional equations and parameters to be inserted into the node. This step is a global transformation that is simplified and modularly defined by using the Silver language feature *collections*. Its mechanism

grammar timeout; import lustre;

prod tmoCondactExpr e::Expr ::= rate::Expr min\_drift::Expr max\_drift::Expr

call::Expr init\_vals::ExprList

{ e.pp = "timeout\_condact(" ++ rate.pp ++ ", " ++ min\_drift.pp ++ ... ; e.typerep = call.typerep ;

e.errors = ...; /\* check that call and init\_vals have the same type \*/ forwards to condactExpr(idExpr(mkTerminal(Id, "fired\_" ++ toString(e.num))),

call, init\_vals); e.num = gen\_unique\_int ( ) ;

/\* gathering information of timeout\_condact calls \*/ e.tmoCallInfoList = [tmoInfo(rate, min\_drift, max\_drift, e.num)]; }

Fig. 5. Silver specification for the *timeout condact* construct.

is not further elaborated here and interested readers may refer to [[13](#_bookmark28)] for detailed explanations.

# Conclusion

* 1. *Discussion*

In this paper we have defined a timeout condact construct useful in specifying and analyzing GALS architectures. It has been implemented as a language extension in an extensible Lustre framework. Timeout automata is one of several approaches for modeling asynchrony within synchronous languages. It has been used successfully on several protocol examples (e.g. [[9](#_bookmark23),[3](#_bookmark18),[4](#_bookmark19)]) and allows a natural expression of inter- esting safety and bounded liveness properties over GALS architectures. However, in the simplistic translation described in this paper, it adds a significant amount of additional state into the model, which makes formal analysis more expensive. Abstractions of the possible real-time evolutions of the architecture, such as those described by [[15](#_bookmark30)] may yield more tractable analysis. The use of extensible languages opens up several possible directions for future research. First, we plan to investigate whether abstractions can be performed as part of the compilation step to “kernel” lustre. Second, we plan on investigating techniques for describing clock relations (such as in [[15](#_bookmark30)]) directly through language extensions.

Our initial efforts in extensible languages were in the domain of programming languages. We have built an extensible specification of Java 1.4 and specified a number of non-trivial language extensions [[29](#_bookmark45)]. One extension embeds the database query language SQL into Java so that queries can be written naturally and syntax and type errors in SQL queries can be detected at compile-time, instead of run-time, as is the case in library-based approaches.

* 1. *Related Work*

There have been many other efforts to extend Lustre with new language features. Many of these features can also be implemented by translation to the a kernel Lustre language. For example, recent work to add state machines to Lustre [[8](#_bookmark21)] translates the state machine constructs into a kernel Lustre language and the addition of modules and generics proposed for Lustre v6.

Extensions for synthesizing Lustre logical clocks from Simulink models with “real-time” rates for blocks are proposed in [[5](#_bookmark20),[6](#_bookmark22)]. This work is similar in that

it moves from a notion of real-time to logical time. Unlike timeout automata, it imposes a fixed real-time value on the base rate of the model; this allows for code generation but makes it more difficult to analyze processes with non-harmonic periods or arbitrarily small amounts of process drift.

Embedded domain specific languages [[16](#_bookmark31)], higher-order extensions to Lustre [[23](#_bookmark38)], and reactive extensions to ML [[19](#_bookmark34)] can be used to build extensible language frame- works for synchronous languages [[7](#_bookmark24)]. But composition of language features typically requires some implementation level understanding of the language extension and thus various extensions cannot be as freely composed as in our approach [[12](#_bookmark27)].

More generally, several approaches have been described for extending languages with new features. Macros systems (lexical, syntactic, hygienic [[18](#_bookmark33)], etc) do al- low new languages constructs to be specified but they lack an effective means for performing the static analysis used to, for example, generate domain specific er- ror messages. Note that some modern macro systems (*e.g.* [[1](#_bookmark17)] however do a some limited facilities for error processing. Object-oriented frameworks, such as Poly- glot [[22](#_bookmark37)], have also been proposed for building extensible languages, but they do not support the automatic composition of language extensions that is provided by the attribute grammar-based approach.

Modular language definition and extensibility has received a significant amount of attention from the AG community. Other attribute grammar approaches lack forwarding and the default definition of attributes that it provides - thus the reuse of language features specified as AG fragments is achieved only by writing attribute definitions that “glue” new fragments into the host language AG. However, a par- ticularly interesting approach is the rewritable reference attribute grammars [[10](#_bookmark25)] in the JastAddII system. New constructs are translated to host language con- structs by destructive rewrites on the syntax tree. Although forwarding is similar to rewriting, it is non-destructive; the original tree and the forwards-to tree exist simultaneously. This allows both the explicit and implicit (via forwarding) speci- fication of semantics, a capability that we have found to be crucial in the highly modular language specifications required for extensible languages and composable language extensions. Some modularity is lost when the rewrites are destructive.

# References

1. Batory, D., D. Lofaso and Y. Smaragdakis, *JTS: tools for implementing domain-specific languages*, in:

*Proc. 5th Intl. Conf. on Software Reuse* (1998).

1. Benveniste, A., P. C. an S. Edwards, N. Halbwachs, P. L. Guernic and R. de Simone, *The synchronous languages 12 years later*, Proceedings of the IEEE 91 (2003), pp. 64–83.
2. Brown, G. M. and L. Pike, *Easy parameterized verification of biphase mark and 8N1 protocols*, in: *Proc. of the 12th International Conference on Tools and the Construction of Algorithms (TACAS’06)*, LNCS 3920 (2006), pp. 58–72.
3. Brown, G. M. and L. Pike, *“Easy” parameterized verificaton of cross clock domain protocols*, in: *Seventh International Workshop on Designing Correct Circuits DCC: Participants’ Proceedings*, 2006, satellite Event of ETAPS.
4. Caspi, P., A. Curic, A. Maigna, C. Sofronis and S. Tripakis, *Translating discrete-time simulink to lustre*, in: *International Conference on Embedded Software (EMSOFT’03)* (2003).
5. Caspi, P., A. Curic, A. Maignan, C. Sofronis, S. Tripakis and P. Niebert, *From simulink to scade/lustre to tta: A layered approach for distributed embedded applications*, in: *LCTES* (2003).
6. Claessen, K. and G. J. Pace, *An embedded language framework for hardware compilation*, in: *Proceedings of Designing Correct Circuits*, 2002.
7. Colaco, J.-L., B. Pagano and M. Pouzet, *A conservative extension of synchronous data-flow with state machines*, in: *Proceedings of the 5th ACM International Conference on Embedded Software* (2005), pp. 173–182.
8. Dutertre, B. and M. Sorea, *Modeling and verification of a fault-tolerant real-time startup protocol using calendar automata*, in: *Formal Techniques in Real-Time and Fault Tolerant Systems*, LNCS 3253, 2004,

pp. 199–214.

1. Ekman, T. and G. Hedin, *Rewritable reference attributed grammars.*, in: *Proc. of ECOOP ’04 Conf.*, 2004, pp. 144–169.
2. *SCADE suite product description—by Esterel technologies.*, [http://www.esterel-technologies.com.](http://www.esterel-technologies.com/)
3. Gao, J., M. Heimdahl and E. Van Wyk, *Flexible and extensible notations for modeling languages*, in:

*Fundamental Approaches to Software Engineering, FASE 2007*, LNCS 4422 (2007), pp. 102–116.

1. Gao, J., M. Heimdahl, M. Whalen and E. Van Wyk, *A flexible and extensible framework for modeling languages*, Technical report, University of Minnesota (2006), available at [www.melt.cs.umn.edu](http://www.melt.cs.umn.edu/).
2. Halbwachs, N., P. Caspi, P. Raymond and D. Pilaud, *The synchronous dataflow programming language Lustre*, Proc. of the IEEE 79 (1991), pp. 1305–1320.
3. Halbwachs, N. and L. Mandel, *Simulation and verification of asynchronous systems by means of a synchronous model*, in: *ACSD 2006, Sixth Intl. Conf. on Application of Concurrency to System Design*, Turku, Finland, 2006.
4. Hudak, P., *Building domain-specific embedded languages*, ACM Computing Surveys 28 (1996).
5. Knuth, D. E., *Semantics of context-free languages*, Mathematical Systems Theory 2 (1968), pp. 127– 145, corrections in 5(1971) pp. 95–96.
6. Kohlbecker, E., D. P. Friedman, M. Felleisen and B. Duba, *Hygienic macro expansion*, in: *Proceedings of the 1986 ACM conference on LISP and functional programming* (1986), pp. 151–161.
7. Mandel, L. and M. Pouzet, *ReactiveML: a reactive extension to ML*, in: *PPDP ’05: Proceedings of the 7th ACM SIGPLAN international conference on Principles and practice of declarative programming* (2005), pp. 82–93.
8. Maraninchi, F. and Y. R´emond, *Mode-automata: About modes and states for reactive systems*, in:

*European Symposium On Programming* (1998).

1. Miller, S. P., M. W. Whalen, D. O’Brien, M. P. Heimdahl and A. Joshi, *A methodology for the design and verification of globally asynchronous/locally synchronous architectures*, Technical Report Contractor Report NASA/CR-2005-213912, NASA (2005).
2. Nystrom, N., M. R. Clarkson and A. C. Myer, *Polyglot: An extensible compiler framework for Java*, in: *Proc. 12th International Conf. on Compiler Construction*, LNCS 2622 (2003), pp. 138–152.
3. Pouzet, M., *Lucid synchrone, version 3. tutorial and reference manual.* (2006), distribution available at: [www.lri.fr/](http://www.lri.fr/~pouzet/lucid-synchrone)∼[pouzet/lucid-synchrone](http://www.lri.fr/~pouzet/lucid-synchrone) .
4. Rocheteau, F. and N. Halbwachs, *Pollux, a Lustre-based hardware design environment*, in: P. Quinton and Y. Robert, editors, *Conference on Algorithms and Parallel VLSI Architectures II*, Chateau de Bonas, 1991.
5. Thompson, J. M., M. P. Heimdahl and S. P. Miller, *Specification based prototyping for embedded systems*, in: *Seventh ACM SIGSOFT Symposium on the Foundations on Software Engineering*, LNCS 1687, 1999.
6. Van Wyk, E., D. Bodin, L. Krishnan and J. Gao, *Silver: an extensible attribute grammar system*, in:

*Proc. of LDTA 2007,* 7*th Workshop on Language Descriptions, Tools, and Analysis*, 2007.

1. Van Wyk, E., O. de Moor, K. Backhouse and P. Kwiatkowski, *Forwarding in attribute grammars for modular language design*, in: *Proc. 11th Intl. Conf. on Compiler Construction*, LNCS 2304, 2002, pp. 128–142.
2. Van Wyk, E. and M. Heimdahl, *Flexibility in modeling languages and tools: A call to arms*, in: *Proc. of IEEE ISoLA Workshop on Leveraging Applications of Formal Methods, Verification, and Validation*, 2005.
3. Van Wyk, E., L. Krishnan, A. Schwerdfeger and D. Bodin, *Attribute grammar-based language extensions for Java*, in: *European Conf. on Object Oriented Programming (ECOOP)*, LNCS 4609 (2007), pp. 575– 599.
4. Vogt, H., S. D. Swierstra and M. F. Kuiper, *Higher-order attribute grammars*, in: *ACM Conf. on Programming Language Design and Implementation (PLDI)*, 1990, pp. 131–145.